United States

site index news servers workstations configure buy technical Tru64 UNIX OpenVMS Linux

compare models

specs user guide service guide graphics drivers firmware updates monitors

Systems and Options Catalog

technical specifications

DIGITAL Personal Workstation au series 433au, 500au, 600au

Performance 433au 500au 600au SPECint_rate_base95 109 123 144 SPECint_rate95 125 142 165 SPECfp_rate_base95 152 162 179 SPECint_rate95 163 175 191

Processors/Chipset Alpha 21164, 433 MHz Alpha 21164, 500 MHz Alpha 21164, 600 MHz Pyxis chipset Memory 6 DIMM sockets support 1.5 GB of ECC SDRAM Cache 96 KB internal cache (L3 cache, 0, 2 MB or 4MB) Disk controller Q-Logic Ultra Wide SCSI, EIDE integrated on MLB (for CD-ROM only) (OpenVMS includes a SCSI CDROM - 12x) Disk 2/4/9 GB 7200 rpm Ultra Wide SCSI Expansion Slots 2 64-bit PCI graphics, 3 PCI/ISA shared Graphics PowerStorm Family Integrated Ethernet 10/100BaseTx-integrated 10BaseT/2-optional PCI 10/100BaseT-optional BIOS 1 MB Flash BIOS Upgrades PowerGrade to 600au Operating System DIGITAL UNIX 4.0d, OpenVMS 7.1-1H1 Mouse/Keyboard PS/2-compatible, 3-button mouse and DIGITAL UNIX or OpenVMS keyboard CD-ROM 24X ATAPI Bus PCI and ISA Bays Internal: two 3.5" (1" form factor (ff)); Front access: three 5.25" (1" or 1.6" ff) and one 3.5" (1" ff) Audio 16-bit Soundblaster-compatible audio integrated on board; five audio ports Power supply 120/240 V External Switchable, single phase, 300 W Enclosure Screwless minitower enclosure with easy access, keylock included Ports Two serial, one parallel, bidirectional ECP/EPP printer port, audio in, audio out, microphone, headset, MDI/joystick.

privacy and legal statement